{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Gas Natural","Combustion"],"not_rendered":{"charts":0,"images":13,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Gas Natural","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[[8,6,8,7]]}
[]
["Gas Natural"]
[]
[]
[null,"Composición"]
[null,null,null,"% Volumen","Fracción volumen renormalizado"]
[null,"Metano","CH4",84.6,{"$f":"D7/$D$26","v":0.75502008032128498}]
[null,"Etano","C2H6",6.4,{"$f":"D8/$D$26","v":5.7117358322177597E-2}]
[null,"Etileno","C2H4",0.8,{"$f":"D9/$D$26","v":7.1396697902721996E-3}]
[null,"Propano","C3H8",0.5,4.4622936189201243E-3,null,null,"yi"]
[null,"Isobutano","C4H10 ",1.2,1.0709504685408298E-2,null,"CH4",{"$f":"E7","v":0.75502008032128498}]
[null,"n-butano","C4H10 ",1.4,1.2494422132976349E-2,null,"C2H6",{"$f":"E8","v":5.7117358322177597E-2}]
[null,"Isopentano","C5H12 ",0.4,3.5698348951360998E-3,null,"H2O",{"$f":"E24","v":0}]
[null,"n-pentano","C5H12 ",0.2,1.7849174475680499E-3,null,"CO2",{"$f":"E18","v":4.4622936189201247E-2}]
[null,"Hexano","C6H14 ",0.4,3.5698348951360998E-3,null,"O2",0]
[null,"Heptano","C7H16 ",0.1,8.9245872378402495E-4,null,"N2 ",{"$f":"E22","v":8.9245872378402494E-2}]
[null,"Hidrógeno","H2",0.2,1.7849174475680499E-3]
[null,"Dióxido de carbono","CO2",5,4.4622936189201247E-2]
[null,"Monóxido de carbono","CO",0.1,8.9245872378402495E-4]
[null,"Helio","He",0.5,4.4622936189201243E-3]
[null,"Sulfuro de hidrogeno","HS",0.2,1.7849174475680499E-3]
[null,"Nitrogeno","N2",10,8.9245872378402494E-2]
[null,"Argon","Ar",0.05,4.4622936189201248E-4]
[null,"Agua","H2O ",0,0]
[null,"No hidrocarburos",null,0,0]
[null,"Total",null,{"$f":"SUM(D7:D25)","v":112.05000000000001}]

{"sheet":"Combustion","index":1,"n_rows":94,"n_cols":10,"rows_kept":94,"cut":false,"hidden":false,"merged":[[3,1,3,2],[83,7,83,8],[56,1,56,8],[70,1,70,8],[36,7,36,8],[37,7,37,8],[83,1,83,2],[83,4,83,5],[20,2,20,3],[20,4,20,5],[20,6,20,7],[36,1,36,2],[36,4,36,5]]}
[]
["Temperatua de flama adiabática"]
[]
[null,"Propieadades termodinámicas"]
[null,"To [K]",{"$f":"25+273.15","v":298.14999999999998}]
[null,"R [J mol-1 K-1]",8.3140000000000001]
[null,"R [kJ mol-1 K-1]",{"$f":"C6/1000","v":8.3140000000000002E-3}]
[null,null,null,null,null,null,null,null,"Δhf o","Δgf o"]
["No. ","Formula ","Name ","a0 ","a1 x 103 ","a2 x 105 ","a3 x 108 ","a4 x 1011 ","kJ / mol ","kJ / mol "]
[26,"CH4 ","methane ",4.5679999999999996,-8.9749999999999996,3.6310000000000002,-3.407,1.091,-74.52,-50.45]
[65,"C2H6 ","ethane ",4.1779999999999999,-4.4269999999999996,5.66,-6.6509999999999998,2.4870000000000001,-83.82,-31.86]
[440,"H2O ","water ",4.3949999999999996,-4.1859999999999999,1.405,-1.5640000000000001,0.63200000000000001,-241.81,-228.42]
[31,"CO2 ","carbon dioxide ",3.2589999999999999,1.3559999999999999,1.502,-2.3740000000000001,1.056,-393.51,-394.38]
[460,"O2 ","oxygen ",3.63,-1.794,0.65800000000000003,-0.60099999999999998,0.17899999999999999,0,0]
[455,"N2 ","nitrogen ",3.5390000000000001,-0.26100000000000001,7.0000000000000001E-3,0.157,-9.9000000000000005E-2,0,0]
[]
[]
[]
[]
[]
[null,null,"Coeficientes Estequiométricos",null,"Reacción 1",null,"Reacción 2"]
[null,null,"Reacción 1","Reacción 2"," α i1 Δhfi [kJ mol-1] "," α i1 Δhgi [kJ mol-1] "," α i2 Δhfi [kJ mol-1] "," α i2 Δhgi [kJ mol-1] "]
[null,"CH4 ",-1,0]
[null,"C2H6 ",0,-1]
[null,"H2O ",2,3]
[null,"CO2 ",1,2]
[null,"O2 ",-2,-3.5]
[null,"N2 ",0,0]
[]
[null,null,"Δhr [kJ mol-1] ","Δgr [kJ mol-1] ","ln K"]
[null,"Reacción 1"]
[null,"Reacción 2"]
[]
[]
[null,"Balance de Materia  en el Mezclador"]
[]
[null,"Aire (Corriente A)",null,null,"Combustible (corriente B)",null,null,"Quemador"]
[null,"T [°C] ",25,null,"T [°C] ",25,null,"Reactor"]
[null,"P[bar]",1,null,"P[bar]",1,null,"%Conversión CH4",100]
[null,"%Exceso de aire",20,null,"Base de cálculo",100,null,"%Conversión C2H6",100]
[null,"yN2",0.79,null,"CH4",0.75502008032128498,null,"Avance reacción 1 (ξ1)"]
[null,"yO2",0.21,null,"C2H6",5.7117358322177597E-2,null,"Avance reacción 2 (ξ2)"]
[null,"yH2O",0,null,"H2O",0,null,"ξ1  Δhr1"]
[null,"NaireEo ",null,null,"CO2",4.4622936189201247E-2,null,"ξ2  Δhr2"]
[null,"NaireE",null,null,"O2",0,null,"Σ ξj  Δhrj"]
[null,null,null,null,"N2 ",8.9245872378402494E-2]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Corriente C=E (entrada al reactor)"]
[null,null,"Flujo","yi","yi a0","yi a1 x 103 ","yi a2 x 105 ","yi a3 x 108 ","yi  a4 x 1011 "]
[null,"CH4"]
[null,"C2H6"]
[null,"H2O"]
[null,"CO2"]
[null,"O2"]
[null,"N2 "]
[null,"Total"]
[null,null,null,null,{"$f":"E65","v":0},{"$f":"F65*0.001","v":0},{"$f":"G65/10^5","v":0},{"$f":"H65/10^8","v":0},{"$f":"I65/10^(11)","v":0}]
[]
[]
[]
[]
[null,"Corriente S (salida del quemador)"]
[null,null,"Flujo","yi","yi a0","yi a1 x 103 ","yi a2 x 105 ","yi a3 x 108 ","yi  a4 x 1011 "]
[null,"CH4"]
[null,"C2H6"]
[null,"H2O"]
[null,"CO2"]
[null,"O2"]
[null,"N2 "]
[null,"Total"]
[null,null,null,null,{"$f":"E79","v":0},{"$f":"F79*0.001","v":0},{"$f":"G79/10^5","v":0},{"$f":"H79/10^8","v":0},{"$f":"I79/10^(11)","v":0}]
[]
[]
[]
[null,"Entrada ( E )",null,null,"Salida (S)",null,null,"Reacción"]
[null,"T [K]",298.14999999999998,null,"T [K]",{"$f":"E94","v":500},null,"Σ ξj  Δhrj"]
[null,"To [K]",{"$f":"C5","v":298.14999999999998},null,"To [K]",{"$f":"C5","v":298.14999999999998}]
[null,"<cp#> [kJ/mol/K]",null,null,"<cp#> [kJ/mol/K]"]
[null,"N<cp#>",null,null,"N<cp#>"]
[null,"N<cp#>(T-To)",null,null,"N<cp#>(T-To)"]
[]
[null,null,null,null,"Balance de energía (ec.10)"]
[]
[null,null,null,null,"T*","Tc (ec. 11)"]
[null,null,null,null,500]