{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Gas Natural","Combustion"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Gas Natural","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[[8,6,8,7]]}
[]
["Gas Natural"]
[]
[]
[null,"Composición"]
[null,null,null,"% Volumen","Fracción volumen renormalizado"]
[null,"Metano","CH4",84.6,{"$f":"D7/$D$26","v":0.75502008032128498}]
[null,"Etano","C2H6",6.4,{"$f":"D8/$D$26","v":5.7117358322177597E-2}]
[null,"Etileno","C2H4",0.8,{"$f":"D9/$D$26","v":7.1396697902721996E-3}]
[null,"Propano","C3H8",0.5,4.4622936189201243E-3,null,null,"yi"]
[null,"Isobutano","C4H10 ",1.2,1.0709504685408298E-2,null,"CH4",{"$f":"E7","v":0.75502008032128498}]
[null,"n-butano","C4H10 ",1.4,1.2494422132976349E-2,null,"C2H6",{"$f":"E8","v":5.7117358322177597E-2}]
[null,"Isopentano","C5H12 ",0.4,3.5698348951360998E-3,null,"H2O",{"$f":"E24","v":0}]
[null,"n-pentano","C5H12 ",0.2,1.7849174475680499E-3,null,"CO2",{"$f":"E18","v":4.4622936189201247E-2}]
[null,"Hexano","C6H14 ",0.4,3.5698348951360998E-3,null,"O2",0]
[null,"Heptano","C7H16 ",0.1,8.9245872378402495E-4,null,"N2 ",{"$f":"E22","v":8.9245872378402494E-2}]
[null,"Hidrógeno","H2",0.2,1.7849174475680499E-3]
[null,"Dióxido de carbono","CO2",5,4.4622936189201247E-2]
[null,"Monóxido de carbono","CO",0.1,8.9245872378402495E-4]
[null,"Helio","He",0.5,4.4622936189201243E-3]
[null,"Sulfuro de hidrogeno","HS",0.2,1.7849174475680499E-3]
[null,"Nitrogeno","N2",10,8.9245872378402494E-2]
[null,"Argon","Ar",0.05,4.4622936189201248E-4]
[null,"Agua","H2O ",0,0]
[null,"No hidrocarburos",null,0,0]
[null,"Total",null,{"$f":"SUM(D7:D25)","v":112.05000000000001}]

{"sheet":"Combustion","index":1,"n_rows":40,"n_cols":12,"rows_kept":40,"cut":false,"hidden":false,"merged":[[5,10,5,11],[5,0,5,7],[16,1,16,2],[16,4,16,5],[31,3,31,4]]}
[]
["Mezclador"]
[]
[null,"To [K]",298.14999999999998]
[]
[null,null,null,null,null,null,null,null,"Δhf o","Δgf o","Coeficientes Estequiométricos"]
["No. ","Formula ","Name ","a0 ","a1 x 103 ","a2 x 105 ","a3 x 108 ","a4 x 1011 ","kJ / mol ","kJ / mol ","Reacción 1","Reacción 2"]
[26,"CH4 ","methane ",4.5679999999999996,-8.9749999999999996,3.6310000000000002,-3.407,1.091,-74.52,-50.45,-1,0]
[65,"C2H6 ","ethane ",4.1779999999999999,-4.4269999999999996,5.66,-6.6509999999999998,2.4870000000000001,-83.82,-31.86,0,-1]
[440,"H2O ","water ",4.3949999999999996,-4.1859999999999999,1.405,-1.5640000000000001,0.63200000000000001,-241.81,-228.42,2,3]
[31,"CO2 ","carbon dioxide ",3.2589999999999999,1.3559999999999999,1.502,-2.3740000000000001,1.056,-393.51,-394.38,1,2]
[460,"O2 ","oxygen ",3.63,-1.794,0.65800000000000003,-0.60099999999999998,0.17899999999999999,0,0,-2,-3.5]
[455,"N2 ","nitrogen ",3.5390000000000001,-0.26100000000000001,7.0000000000000001E-3,0.157,-9.9000000000000005E-2,0,0,0,0]
[]
[]
[]
[null,"Aire (Corriente A)",null,null,"Combustible (corriente B)"]
[null,"T [°C] ",25,null,"T [°C] ",25]
[null,"P[bar]",1,null,"P[bar]",1]
[null,"%Exceso de aire",20,null,"Base de cálculo",100]
[null,"yH2O",0,null,"CH4",0.79811320754716986]
[null,"yO2",0.21,null,"C2H6",6.0377358490566045E-2]
[null,"yN2",0.79,null,"H2O",0]
[null,null,null,null,"CO2",4.716981132075472E-2]
[null,null,null,null,"O2",0]
[null,null,null,null,"N2 ",9.4339622641509441E-2]
[]
[]
[]
[]
[null,"Balance de Materia  en el Mezclador"]
[null,null,null,"Referencia",null,"Calculado"]
[null,"ID","Sustancia","Flujo","yi","yi"]
[null,1,"CH4",79.811320754716988,7.0449678800856536E-2,{"$f":"Mezclador(B34,$C$18:$C$23,$F$18:$F$26)","v":7.0449678800856522E-2}]
[null,2,"C2H6",6.0377358490566042,5.3295265286699978E-3,{"$f":"Mezclador(B35,$C$18:$C$23,$F$18:$F$26)","v":5.3295265286699969E-3}]
[null,3,"H2O",0,0,0]
[null,4,"CO2",4.716981132075472,4.1636926005234358E-3,4.1636926005234349E-3]
[null,5,"O2",216.90566037735849,0.19146324054246966,0.19146324054246966]
[null,6,"N2 ",825.41239892183296,0.7285938615274804,0.72859386152748051]
[null,7,"Total",1132.8840970350404,1,1132.8840970350407]