{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Hoja1","Hoja2","Hoja3"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":17,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoja1","index":0,"n_rows":73,"n_cols":21,"rows_kept":73,"cut":false,"hidden":false,"merged":[[55,6,55,7],[0,4,0,15],[1,16,1,17],[11,1,11,2],[11,4,11,5],[25,2,25,3],[41,2,41,3],[25,5,25,6],[25,8,25,9],[41,6,41,7]]}
[null,null,null,null,"Propiedades"]
[null,"To [K]",298.14999999999998,null,1,2,3,4,5,6,7,8,9,10,11,12,"Coeficientes Estequiométricos",null,13,14,15]
["Name ","No. ","Formula ","Trange, K ","A","B × 103 ","C × 105","D × 108","E × 1011","Tc (K)","Pc (bar)","Vc (cm3/mol)","Zc","ω","Δhfo[kJ mol-1 ]","Δgfo[kJ mol-1 ]","Reacción 1","Reacción 2","A","B","C"]
["Metano",26,"CH4 ","50-1000 ",4.5679999999999996,-8.9749999999999996,3.6310000000000002,-3.407,1.091,190.56,45.99,98.6,0.28600000000000003,1.0999999999999999E-2,-74.52,-50.45,-1,0,3.7686999999999999,395.74400000000003,266.68099999999998]
["Etano",65,"C2H6 ","50-1000 ",4.1779999999999999,-4.4269999999999996,5.66,-6.6509999999999998,2.4870000000000001,305.32,48.72,145.5,0.27900000000000003,9.9000000000000005E-2,-83.82,-31.86,0,-1,3.9540500000000001,663.72,256.68099999999998]
["Agua",440,"H2O ","50-1000 ",4.3949999999999996,-4.1859999999999999,1.405,-1.5640000000000001,0.63200000000000001,647.14,220.64,55.95,0.22900000000000001,0.34400000000000003,-241.81,-228.42,2,3,5.11564,1687.537,230.17]
["Dióxido de carbono",31,"CO2 ","50-1000 ",3.2589999999999999,1.3559999999999999,1.502,-2.3740000000000001,1.056,304.12,73.739999999999995,94.07,0.27400000000000002,0.22500000000000001,-393.51,-394.38,1,2,0,0,0]
["Oxígeno",460,"O2 ","50-1000 ",3.63,-1.794,0.65800000000000003,-0.60099999999999998,0.17899999999999999,154.58000000000001,50.43,73.37,0.28800000000000003,0,0,0,-2,-3.5,3.8163400000000003,319.01299999999998,266.7]
["Nitrógeno",455,"N2 ","50-1000 ",3.5390000000000001,-0.26100000000000001,7.0000000000000001E-3,0.157,-9.9000000000000005E-2,126.2,33.979999999999997,90.1,0.28899999999999998,3.6999999999999998E-2,0,0,0,0,3.6194700000000002,255.68,266.55]
[]
[]
[null,"Aire (Corriente A)",null,null,"Combustible (corriente B)"]
[null,"T [°C] ",25,null,"T [°C] ",25,null,"Conversión CH4",100]
[null,"P[bar]",1,null,"P[bar]",1,null,"Conversión C2H6",100]
[null,"%Exceso de aire",20,null,"Base de cálculo[mol/h]",100]
[null,"yH2O",0,null,"CH4",0.79811320754716986]
[null,"yO2",0.21,null,"C2H6",6.0377358490566045E-2]
[null,"yN2",0.79,null,"H2O",0]
[null,null,null,null,"CO2",4.716981132075472E-2]
[null,null,null,null,"O2",0]
[null,null,null,null,"N2 ",9.4339622641509441E-2]
[]
[]
[]
[]
[null,"ID","Mezclador ( C )",null,null,"Aire (Corriente E)",null,null,"Compresor (Corriente F)"]
[null,null,"T [K]",298.14999999999998,null,"T [°C] ",298.14999999999998,null,"T [°C] "]
[null,null,"P[bar]",1,null,"P[bar]",1,null,"P[bar]",20]
[null,1,"y CH4",null,null,"y CH4",0,null,"s [kJ mol -1 K-1]"]
[null,2,"y C2H6",null,null,"y C2H6",0,null,"y CH4"]
[null,3,"y H2O",null,null,"y H2O",0,null,"y C2H6"]
[null,4,"y CO2",null,null,"y CO2",0,null,"y H2O"]
[null,5,"y O2",null,null,"y O2",0.21,null,"y CO2"]
[null,6,"y N2 ",null,null,"y N2 ",0.79,null,"y O2"]
[null,7,"Total [mol/h]",null,null,"%Exceso de aire",377,null,"y N2 "]
[null,8,"Aire  teo [mol/h]",null,null,"Total [mol/h]",null,null,"Total [mol/h]"]
[null,null,null,null,null,"s [kJ mol -1 K-1]",null,null,"h [kJ mol -1]"]
[null,null,null,null,null,"h [kJ mol -1]",null,null,"W [kW]"]
[]
[]
[]
[null,"ID","Quemador (D)",null,null,"ID","Mezclador ( G )"]
[null,1,"T f adiabática [K]",null,null,null,"T [K]"]
[null,2,"Error",null,null,1,"P[bar]"]
[null,3,"Qmax [kJ / h]",null,null,2,"h [kJ mol -1]"]
[null,4,"yCH4 ",null,null,3,"y CH4"]
[null,5,"yC2H6 ",null,null,4,"y C2H6"]
[null,6,"yH2O ",null,null,5,"y H2O"]
[null,7,"yCO2 ",null,null,6,"y CO2"]
[null,8,"yO2 ",null,null,7,"y O2"]
[null,9,"yN2 ",null,null,8,"y N2 "]
[null,10,"Total [mol/h]",null,null,9,"Total [mol/h]"]
[null,null,null,null,null,null,"s [kJ mol -1 K-1]"]
[null,null,"To [K]",298.14999999999998]
[null,null,"P[bar]",1]
[null,null,"h entrada [kJ/mol]",{"$f":"hmez(D54,D55,D46:D51,E4:P9)","v":0},null,"ID","Turbina ( H )"]
[null,null,null,null,null,null,"T [K]"]
[null,null,"Eficiencia",70,null,null,"P[bar]",1]
[null,null,"Qreal [kJ / h]",null,null,null,"s [kJ mol -1 K-1]"]
[null,null,"Treal [K]",null,null,null,"y CH4"]
[null,null,"hreal [kJ/mol]",null,null,null,"y C2H6"]
[null,null,null,null,null,null,"y H2O"]
[null,null,null,null,null,null,"y CO2"]
[null,null,null,null,null,null,"y O2"]
[null,null,null,null,null,null,"y N2 "]
[null,null,null,null,null,null,"Total [mol/h]"]
[null,null,null,null,null,null,"h [kJ mol -1]"]
[null,null,null,null,null,null,"W [kW]"]
[]
[]
[]
[]
[null,null,null,null,null,null,"W neto [kW]"]

{"sheet":"Hoja2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Hoja3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}